
1. Prepare the BIST file  
  - Copy attachment to USB memory stick and unzip it  
2. Copy the BIST folder (see directory tree below)  
    
3. Run BIST  
  - Connect the USB memory stick to the SPC-7000 and boot  
  - Check if BIST FOR SPC7000 is displayed on the LCD screen  
4. Execute factory reset command  
  - Set PC IP address to 192.168.1.XXX  
  - Execute the following factory reset command from the web browser  
  - URL: <http://192.168.1.100/cgi-bin/adv/factory.cgi?operation=5>  
  - Check if OK is displayed in web browser  
5. Reboot  
  - SPC-7000 Reboot  
  
※ Caution: Executing the above command initializes all device, user and password information set in SPC-7000.